Best WAP sites

this technique is tested on 6600 & 7610
SETUP FREE GPRS ON AIRTEL CONNECTION :
U MUST HAVE AIRTEL LIVE ACTIVATED.
SETTINGS :
1. OPEN REAL ONE PLAYER-OPTIONS-SETTINGS-CONNECTION-NETWORK
DEFAUT ACCESS POINT=AIRTEL LIVE
ONLINE TIME UNLIMITED
MAXIMUM BANDWIDTH=40.2KBPS
CONNECTION TIME-OUT=60 SECS.
SERVER TIME-OUT=40SECS.LOWEST UDP PORT=6970
HIGHEST UDP PORT=32000
NOW GO BACK-BACK-BACK-EXIT.
2. OPEN SERVICES-OPTIONS-SETTINGS-
DEFAULT ACCESS POINT-OPTIONS-NEW ACCESS POINT-
USE EXISTING SETTINGS-AIRTEL LIVE-SELECT-
CONNECTION NAME-MOBILE-HUNGAMA
HOMEPAGE=HTTP://TAGTAG.COM/MOBILE-HUNGAMA
NOW GO BACK AND SELECT MOBILE-HUNGAMA
AND GO BACK.
3. OPEN SERVICES AGAIN-OPTIONS-BOOKMARK MANAGER-
ADD BOOKMARK-NAME=cnbc-
ADDRESS=rtsp://100.1.200.213/rtpencoder/cnbc.sdp
access point=airtel live
options-save
now u have done it.
restart ur handset.